REQUIREMENTS:

Design a controller (P, PI, PD or PID) to achieve following goals

* • Rise time < 5 s
* • Overshoot < 10%
* • Steady-state error < 2%